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Columns 1-2 should be completed by the contracting authority
Columns 3-4 should be completed by the tenderer
Column 5 is reserved for the evaluation committee 
Annex III - the contractor's technical offer
The tenderers are requested to complete the template on the next pages: 
· Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer), 
· Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)  
· Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation
The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.
The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offered specifications.




	1.
Item number
	2.
Specifications required
	3.
Specifications offered
	4. 
Notes, remarks, 
ref to documentation
	5.
Evaluation committee’s notes

	1. 
	Ergonomic L-Shaped Workstation
A commercial-grade, fixed-height (750 mm) Ergonomic L-Shaped Workstation featuring a main desk surface of 1600 mm (L) × 700–800 mm (D) and a reversible return extension measuring 1200–1500 mm (L) × 600–700 mm (D). the L-shape workstation must be constructed from moisture-resistant, minimum 25 mm thick HDF or MFC finished with a machine-bonded 2 mm PVC/ABS edge banding and a low-glare, matte finish to minimize eye strain from overhead office lighting. The colour scheme must be either a Modern Minimalist Dual-Tone (Matte Charcoal Grey or Solid White desktop paired with a Powder-Coated Black steel frame) or a Premium Executive Dual-Tone (Deep Oak or Modern Walnut woodgrain desktop paired with a Powder-Coated Graphite Grey or Black steel frame). The structure must be supported by a heavy-duty steel frame (minimum 1.5 mm wall thickness) with a square or T/C-leg profile, under-desk anti-sag support rails, a static load capacity of 100 kg, and adjustable levelling feet (+ or -15{ mm) to compensate for uneven flooring, complete with at least two pre-drilled 60 mm} cable grommet holes with matching aluminium or plastic flip-top caps.
Quantity: 1 pc

	
	
	

	2. 
	Executive Bow-Top Desk (1.4m)
 Executive Bow-Top Desk measuring 1400 mm (W) × 750 mm (H), featuring a curved desktop that smoothly tapers from 850 mm depth at the centre to 750 mm at the edges to provide a comfortable front visitor overhang. Constructed from durable, moisture-resistant 25–36 mm thick MFC or HDF, the workstation must feature a premium, low-glare matte woodgrain laminate finish—strictly specified as Dark Walnut, Modern Walnut, or Modern Walnut with contrasting Dust Grey/Graphite accents—with machine-bonded 2 mm matching PVC edge-banding and a full-height 18 mm structural modesty panel. The unit must incorporate an integrated 3-drawer pedestal cabinet equipped with full-extension steel ball-bearing glides, adjustable hanging file rails for A4/Legal documents, a central cylinder lock with two keys, and heavy-duty adjustable nylon levelling feet (+ or -15{mm}) to ensure absolute stability on uneven flooring.
Quantity: 2 pcs

	 
	
	

	3. 
	8-10 Seater Meeting Table (2.4m)
A heavy-duty, commercial-grade 8–10-seater Meeting Table measuring 2400 mm (L) × 1200 mm (W) × 750 mm (H). The tabletop must be constructed from moisture-resistant, 25–36 mm thick HDF or MFC featuring a low-glare, matte scratch-resistant laminate finish explicitly specified in a professional Dark Walnut, Cherry, or Modern Oak woodgrain, sealed with machine-bonded 2 mm PVC edge banding. The unit must be supported by a corrosion-resistant, powder-coated heavy-duty steel frame or reinforced panel structure equipped with dual anti-sag support beams and adjustable nylon levelling feet (+ or -15mm}). For clean connectivity, the table must feature two integrated centre-line aluminium flip-top cable grommets with under-desk wire routing tracks, delivered in secure flat-pack packaging suitable for standard commercial assembly.
Quantity: 2 pcs
	 
	
	

	4. 
	Executive Ergonomic High-Back Chair
The seat cushion must feature an ergonomic, sag-resistant High-Density Virgin Molded Polyurethane Foam (Minimum 50kg/m^3 density) upholstered in premium, abrasion-resistant fabric, while the backrest must be constructed from high-tensile, breathable mesh with an integrated headrest and adjustable lumbar support. the colour scheme shall be : Matte Black (All Components): Black mesh, black seat upholstery, and black armrest pads on a black/charcoal frame or Dark Gray Accent Option: Charcoal Dark Gray mesh and seat fabric with a matte black frame.
The mechanical framework must include 3D adjustable armrests with soft PU pads, a multi-position lock synchro-tilt mechanism, and a heavy-duty Class 4 pneumatic gas lift rated for a minimum weight capacity of 130 kg. To withstand the high humidity and salinity of Bossaso's coastal environment, the chair base must be explicitly constructed from rust-proof Die-Cast Aluminium or reinforced heavy-duty Nylon (Steel chrome bases are strictly excluded to prevent corrosion) forming a 680 mm five-star footprint, equipped with 60mm dual-wheel polyurethane casters, and shipped flat-packed with all assembly tools included.
Quantity: 1 pc
	
	
	

	5. 
	Office Chair, Mid-Back Ergonomic Task Chair
Mid-Back Ergonomic Task Chair configured to support general staff operations, finished uniformly in Matte Black or Dark Gray. The seat cushion must utilize high-resiliency molded polyurethane foam (Minimum 40–50 kg/m³ density) upholstered in an abrasion-resistant, easy-to-clean commercial fabric, paired with a high-tensile breathable mesh backrest featuring integrated lumbar support. The chair must include heavy-duty polypropylene (PP) T-armrests, a smooth pneumatic gas lift height adjustment mechanism with 360-degree swivel, and a canter-tilt lock system rated for a minimum weight capacity of 120 kg. To ensure climate resilience against coastal humidity and salinity, the foundation must consist of a high-strength reinforced Nylon five-star base (Minimum 640mm) equipped with 50mm dual-wheel hooded casters, delivered flat-packed with all necessary assembly hardware.
Quantity: 3 pcs
	
	
	

	6. 
	Ergonomic Sled-Base Meeting Chair
Ergonomic Sled-Base Meeting Chair engineered specifically for boardroom deployment, finished uniformly in Matte Black or Charcoal Dark Gray. The base structure must be constructed from continuous, non-bending tubular cold-rolled steel (minimum 25mm with 1.8 mm wall thickness) coated in an anti-corrosive, matte powder finish and fitted with non-marking nylon anti-scratch glides. The seat must feature an ergonomic waterfall edge utilizing High-Density Virgin Molded Polyurethane Foam (Minimum 45–50 kg/m³ density), paired with a high-tensile breathable mesh backrest with built-in lumbar contours and integrated steel armrests with soft PP/PU pads. The chair frame and base geometry must include an engineered anti-tip rear lean certified to support a structural load capacity of at least 130 kg, delivered in nested or secure commercial flat-pack batches.
Quantity: 20 pcs
	
	
	

	7. 
	3-Door Wooden Filing Cabinet
A heavy-duty, commercial-grade 3-Door Wooden Filing Cabinet / Credenza measuring 1200–1400 mm (W) × 400–450 mm (D). The unit's main chassis and door fronts must be constructed from moisture-resistant, minimum 18 mm thick MFC or MDF, while the top load-bearing surface must be a minimum 25 mm thick. To ensure structural stability and dustproofing in coastal environments, the cabinet must incorporate a solid 9–12 mm thick backing panel. The surface must feature a low-glare, scratch-resistant matte woodgrain finish strictly specified as Dark Walnut or Modern Walnut with machine-bonded 2 mm PVC edge-banding. Internally, the unit must feature adjustable shelves rated for 35 kg each with anti-slip steel pins. The doors must be mounted on heavy-duty soft-close concealed metal hinges, include brushed aluminium handles, feature a secure cylinder lock with two keys, and be supported by adjustable nylon leveling feet (+ or - 15mm) to compensate for uneven office flooring.
Quantity: 3 pcs
	
	
	

	8. 
	Desktop Computers (All-in-One) desk
An All-in-One (AIO) desktop computer featuring a second-generation Intel Core i5 processor (released around 2011–2012) is built on the "Sandy Bridge" architecture, typically delivering base speeds between 2.5GHz and 3.1 GHz across 4 physical cores. Standard configurations from this era generally feature a 23-inch Full HD (1920 X 1080) display, 8 GB of expandable DDR3 RAM, and an integrated Intel HD 2000/3000 graphics chip. For storage and connectivity, a 500 GB to 1 TB mechanical hard drive, a built-in DVD burner, multiple USB 2.0 ports, a 720p webcam, and integrated Gigabit Ethernet alongside 2.4 GHz Wi-Fi.
Quantity: 5 pcs
	
	
	

	9. 
	Laptop Computers

12th or 13th Generation Intel Core i7 processors (utilizing a hybrid architecture with up to 10 or 14 cores) paired with 16GB of high-speed dual-channel DDR4 or LPDDR5 RAM and a lightning-fast 512GB to 1TB PCIe NVMe M.2 Solid State Drive (SSD). Designed for maximum versatility and professional mobility, these laptops feature a vibrant 13.3-inch to 15.6-inch Full HD (1920 × 1080) or WUXGA IPS touchscreen mounted on a robust 360-degree geared hinge that effortlessly flips from laptop to tablet mode, to support an active digital stylus pen. Encased in a durable, sleek aluminium chassis built to meet rigid durability standards, the system comes fully optimized for modern corporate environments with integrated Intel Iris Xe Graphics, a high-definition infrared privacy webcam with an electronic shutter, a backlit spill-resistant keyboard, a fingerprint reader, and premium wireless connectivity via Wi-Fi 6E and Bluetooth 5.3. For comprehensive peripherals handling, the hardware includes dual Thunderbolt 4 / USB-C ports with Power Delivery and DisplayPort capabilities, standard USB 3.2 Type-A ports, an HDMI 2.1 output, a long-lasting 3-to-4 cell lithium-ion battery with fast-changing technology, and comes pre-installed with an enterprise-ready, fully compliant Windows 11 Pro 64-bit operating system.

Quantity: 5 pcs
 
	
	
	

	10. 
	Multifunction Office Printer, scanning, and copying, FS-1025 MFP 
Detail: 
Main Functions: Print, Copy, and Color Scan
Processor / CPU: ARM 390 MHz
Memory: 64 MB RAM (Standard)
Control Panel: 2-line LCD / LED display
Standard Interfaces: High-Speed USB 2.0, Fast Ethernet (10/100BaseTX) for network sharing
Warm-up Time: Approx. 23 seconds or less from power on
Monthly Duty Cycle: Maximum 20,000 pages per month
Dimensions (W x D x H): 390 × 361 × 362 mm
Weight: Approx. 10.0 kg
Quantity: 1 pc
	
	
	

	11. 
	Photocopying machine (High-volume print/copy, Canon 2224i or equivalent)
Machine Type: A3 Monochrome Laser Multifunctional (Print, Copy, Scan, Send).
Performance Speed: Up to 24 ppm (A4) and 12 ppm (A3); First-Copy-Out Time of 7.4 seconds or less.
Resolution Quality: Up to 1200 X 1200\ dpi (Printing) / 600 X 600 dpi (Copying/Scanning).
Processing Power: 1.6GHz Dual-Core Processor with 1.0 GB RAM and 2 GB eMMC internal storage.
User Interface: 8.9 cm (3.5 inch) Monochrome LCD Touch Panel.
Job Handling Capacity: Continuous copying from 1 to 999 sheets with a 25% to 400% zoom range (1% steps).
Paper Capacity: Standard 350 sheets (250-sheet Cassette + 100-sheet Multi-purpose Tray), expandable up to 600 sheets.
Media Handling: Supports sizes from A5 to A3; weights from 64–90 gsm (Cassette) and 60–157 gsm (Bypass Tray).
Consumables & Economy: Uses Canon C-EXV 42 Black Toner with a high-yield capacity of up to 10,200 pages (at 5% coverage).
Digital Workflow Tools: Features electronic collation, N-on-1 layout creation, ID Card/Passport Copy mode, and border frame erase.
Quantity: 2 pcs

	
	
	

	12. 
	Multifunction Projector (EPSON or equivalent)
Details
· A 3LCD Multifunction Business Projector is a premium corporate-grade projection system featuring a native 3-chip liquid crystal shutter mechanism that ensures matching white and color light outputs up to 4,000 to 4,500 ANSI Lumens. 
· Delivering crisp text and vibrant widescreen graphics at a native Full HD (1920 × 1080) or WUXGA (1920 × 1200) resolution, the optical assembly features a 1.2x to 1.6x manual zoom, a sharp 16,000:1 contrast ratio, and a dual-axis keystone correction framework (pm30 circ vertical and horizontal) with Quick Corner digital edge alignment. 
· Engineered for PC-free, high-collaborative workspaces, its advanced interface incorporates dual HDMI ports, a USB Type-A port for independent flash drive media playback, and robust network modules including a wired RJ-45 Gigabit Ethernet port alongside integrated Wi-Fi and Miracast screen mirroring for wireless multi-device casting via the Epson or equivalent  iProjection application.
·  Accompanied by an internal 10W to 16W speaker, standard 220-240V power grids compatibility, and an ultra-quiet 28 dB economy profile, its light engine offers exceptional operational durability spanning up to 12,000 hours on UHE lamps or 20,000 maintenance-free hours on advanced laser configurations.
Quantity: 2 pcs


	
	
	

	13
	Tripod Projector Screens (70" x 70" (180cm x 180cm)
Viewing Dimensions: Active screen size of 180cm x 180cm (70" x 70") with a 90-inch diagonal display footprint.
Aspect Ratio Flexibility: Native 1:1 square format that easily adjusts vertically to accommodate 4:3, 16:9, and 16:10 video layouts.
Fabric & Optical Gain: Premium Matte White multi-layer fabric featuring a 1.0 to 1.1 Gain rating to eliminate canter hot-spotting.
Viewing Angle: Ultra-wide 160° effective viewing angle, ensuring clear text legibility for participants seated on the sides of the room.
Light Blocking & Contrast: Standard light-blocking black backing prevents rear light penetration, framed by 30mm black masking borders to enhance image contrast.
Structural Framework: Sturdy, heavy-duty steel or aluminum tripod base equipped with non-slip rubber feet and an integrated keystone eliminator tilt mechanism.
Casing & Roll System: Scuff-resistant, powder-coated steel octagonal housing with a smooth, heavy-duty internal spring roller for manual retraction.
Portability: Engineered under 10 kg with an ergonomic carrying handle and an automatic safety lock to keep the tripod legs secured during transit.
Quantity: 2 pcs
	
	
	

	14
	65-Inch Smart TV  (UHD/ThinQ)
Display Footprint: 65-inch native diagonal screen size with a standard 16:9 widescreen aspect ratio. Resolution & Motion: Ultra High Definition (4K UHD, 3840 × 2160 pixels) driven by a native 60 Hz refresh rate.
Contrast & Image Processing: Multi-format HDR support (including HDR10 and HLG) featuring an integrated AI 4K upscaling engine (or equivalent) to intelligently enhance low-resolution training media. Smart Infrastructure: Open-architecture smart TV operating system with an intuitive user interface, voice-control remote capability, and ecosystem compatibility like Apple AirPlay 2 (or equivalent).
Wireless Networking: Dual-band Wi-Fi 5 or Wi-Fi 6 (2.4 GHz / 5 GHz) and Bluetooth 5.0 (or equivalent) for wireless peripherals. Screen Mirroring: Built-in peer-to-peer casting protocols (Miracast, Windows Wireless Display, or equivalent) for wireless laptop-to-screen presentations.
Physical Connections: Minimum 3 × HDMI ports (including 1 × eARC/ARC port), 2 × USB Type-A ports for direct drive media playback, 1 × Digital Optical Audio out, and 1 × RJ-45 Ethernet network port. Audio System: Integrated chassis speakers delivering a minimum of 20W total output with intelligent environmental audio tuning (or equivalent).
Mounting & Power Compliance: Standard VESA 300 mm × 300 mm wall-mount layout; fully compliant with standard AC 220–240V, 50/60Hz power grids.  Energy Management: Built-in ambient light sensor for automatic brightness adjustment and an eco-sleep timer to prevent power waste.
Quantity: 2 pcs

	
	
	

	15
	Ancillary Services -Installation and Maintenance 
The contractor shall provide all ancillary services necessary for the full delivery and operational use of the supplied items, including but not limited to:
· Delivery to the designated site; 
· Assembly and installation; 
· Configuration and positioning where applicable; 
· Testing and commissioning after installation; 
· Preventive and corrective maintenance during the warranty period; 
· Replacement or repair of defective components during the warranty period. 
The contractor shall ensure that all supplied items are fully operational upon completion of installation.
All costs related to supply, transportation, delivery, labour, installation, maintenance, warranty services, tools, equipment, and any other incidental expenses shall be included in the financial offer.
No separate payment shall be made for ancillary services not explicitly priced separately in the financial offer.
During the warrant period maintenance of items is upon supplier 

	
	
	




Additional requirements:
Note: The contractor is required to provide a minimum 12-month commercial warranty for all electronic equipment (computers, printers, etc.) and ensure physical delivery and placement within the designated office rooms at the PAG headquarters in Bossaso.
All prices are to be quoted DAP Bossaso, Puntland Attorney General’s Office. 
1. Delivery: 30 days from receiving the Order Form.
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