Market TACTICAL EQUIPMENT

TECHNICAL SPECIFICATIONS

Version UPDATED 13 01 2025

TECHNICAL SPECIFICATIONS

See standard form below

ANNEX II + III: TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title:** SUPPLY OF SECURITY EQUIPMENT

Publication reference:

Columns 1-2 to be completed by the contracting authority

Columns 3-4 to be completed by the tenderer

Column 5 reserved for the evaluation committee

Annex III – The contractor’s technical tender

Tenderers must complete the following model:

* Column 2, completed by the contracting authority, specifies the specifications requested (not to be modified by the tenderer),
* Column 3 must be completed by the tenderer and must detail the tender (the use of the words “compliant” and “yes” is insufficient in this respect)
* Column 4 allows tenderers to comment on their supply offer and possibly makedocumentary references

Any documentation provided must clearly indicate (underlined, remarks) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Tenders which do not accurately identify the models and specifications may be rejected by the evaluation committee.

The tender must be sufficiently clear to allow evaluators to easily make a comparison between the requested specifications and the proposed specifications.

**LOT 1: Supply and Delivery of Security Equipment to Beninese law enforcement forces**

| 1.  Article number | 2  Specifications required (+ quantity required) | 3  Proposed specifications | 4  Notes, remarks,  Documentation reference | 5  Notes from the Evaluation Committee |
| --- | --- | --- | --- | --- |
| 1.1 | BALISTIC KNIVES   * Ballistic shield class III+ / IV * Individual * With window * Level min. III * Weight: approx. 18 kg (+/- 10%) * Colour: black   QUANTITY: 20  DELIVERY COTTONOU / BENIN |  |  |  |
| 1.2 | WINE BRISES   * Transportable and compact tool for breaking vehicle windows   QUANTITY: 5  DELIVERY COTTONOU / BENIN |  |  |  |
| 1.3 | COUPANT PINCES   * Bolt cutter * Powerful head * Drowning joint, with eccentric double-joint construction * Black and cold browned surface, polished head, plastic coated branches * Subject(s): Chromium-vanadium steel, forged and hardened * Cutting capacity: soft yarn up to ⁇ : 5,5 mm, hard wire up to ⁇ : 3.2 mm * Total length 300 mm (+/- 15%) * Handle with plastic coating   QUANTITY: 1  DELIVERY COTTONOU / BENIN |  |  |  |
| 1.4 | SAC A MUNITIONS   * Must be foldable and wear to the belt * Must measure H10cm x L10cm x P5cm (+/- 10%) when the pocket is folded * Must measure 20 cm (+/- 10%) in opening and between 25 and 30 cm (+/- 10%) in height when unfolded * Must be made of resistant cordura fabric of Coyote or olive green color * Must have a clamping system at the opening to prevent objects from falling out of the bag * Must have a velcro flap to keep it closed to the belt   **QUANTITY:**  **2**  DELIVERY COTTONOU / BENIN |  |  |  |

**LOT 2: Lot 2 – Supply and Delivery of Security Equipment to Republic Cote d’Ivoire law enforcement forces**

| 1.  Article number | 2  Specifications required (+ quantity required) | 3  Proposed specifications | 4  Notes, remarks,  Documentation reference | 5  Notes from the Evaluation Committee |
| --- | --- | --- | --- | --- |
| 2.1 | EXERCISE SUBMISSION   * Of metal * Handcuff holder with safety clip closure: included * Handcuffs adaptable to all types of wrists * A chains * Colour blue   QUANTITY: 15  ABIDJAN DELIVERY / COTE D’IVOIRE |  |  |  |
| 2.2 | AK 47 BLUE GUNS   * Standard model * Polyurethane, very resistant plastic * With internal metal frame to respect the balance of the weapon * Usable in all climatic conditions (cold, hot, dry, humid...) * Colour blue   QUANTITY: 10  ABIDJAN DELIVERY / COTE D’IVOIRE |  |  |  |
| 2.3 | PA BLUE GUNS   * Standard model * Polyurethane, very resistant plastic * With internal metal frame to respect the balance of the weapon * Colour blue * Usable in all climatic conditions (cold, hot, dry, humid...)   QUANTITY: 10  ABIDJAN DELIVERY / COTE D’IVOIRE |  |  |  |
| 2.4 | TRAINING HANDLE   * Standard model * Polyurethane, very resistant plastic * With internal metal frame to respect the balance of the weapon * Colour blue * Usable in all climatic conditions (cold, hot, dry, humid...)   QUANTITY: 10  ABIDJAN DELIVERY / COTE D’IVOIRE |  |  |  |
| 2.5 | TRAINING BATON (LOT PN)   * Standard model * Light baton for self-defence training * Color blue or black * Hard plastic with padded foam for shock absorption * • length: 50 cm (+/- 10%) * • diameter: 4 cm (+/- 10%) * Usable in all climatic conditions (cold, hot, dry, humid...)   QUANTITY: 10  ABIDJAN DELIVERY / COTE D’IVOIRE |  |  |  |
| 2.6 | BALISTIC KNIVES   * Ballistic shield class III+ / IV * Individual * With window * Level min. III * Weight: approx. 18 kg (+/- 10%) * Colour: black   QUANTITY: 5  ABIDJAN DELIVERY / COTE D’IVOIRE |  |  |  |
| 2.7 | SAC A MUNITIONS   * Must be foldable and wear to the belt * Must measure H10cm x L10cm x P5cm (+/- 10%) when the pocket is folded * Must measure 20 cm (+/- 10%) in opening and between 25 and 30 cm (+/- 10%) in height when unfolded * Must be made of resistant cordura fabric of Coyote or olive green color * Must have a clamping system at the opening to prevent objects from falling out of the bag * Must have a velcro flap to keep it closed to the belt   **QUANTITY:**  **2**  ABIDJAN DELIVERY / COTE D’IVOIRE |  |  |  |
| 2.8 | **AK TRIPLE CHARGER DOORS**   * Triple loader holder MOLLE fastening system for long guns to be adapted on plate holder * Cordura/nylon/polyester * 3 pockets of equal sizes with drainage eyelet on the bottom * Capacity of 3 AK47 chargers * Velcro closure on the top * Fastening by soft fastener * Velcro flap and elastic retention of chargers * Attachment: Molle Passersby * Colour: Coyote or olive green   QUANTITY: 30  ABIDJAN DELIVERY / COTE D’IVOIRE |  |  |  |
| 2.9 | HOLSTERS   * Universal/polyvalent compatible automatic gun * In Cordura * Safety placket with push button * Omnivorous model compatible Norinco NP 22 and Tokarev TT33 * Ergonomics * Fastening: belt * Ambidextrous * Colour: Black   QUANTITY: 50  ABIDJAN DELIVERY / COTE D’IVOIRE |  |  |  |
| 2.10 | ORDER MAINTENANCE TACTICAL GILET   * Fabric: High-tenacity polyamide or high-strength nylon net. * Press buttons: Brass/plastic * Extraction handle * Location for identifier * Multi-pass backbone for attaching clip accessories * Adjustments of the modular intervention chasuble * Shoulders padded. * Elastic cords on both sides * MOLLE system for fixing multiple devices * Removable accessory pockets and doors * Various storage pockets (phone, stick, cartridges, aerosol, etc.)   QUANTITY: 50  ABIDJAN DELIVERY / COTE D’IVOIRE |  |  |  |
| 2.11 | HOSE DOOR   * Strap: Polypropylene or equivalent * Pressure: Brass/Plastic * Strap flap with snap button * Straps from belt to strap * Passing 50mm (+/- 10%)   QUANTITY: 250  ABIDJAN DELIVERY / COTE D’IVOIRE |  |  |  |
| 2.12 | MAINTENANCE CASE OF THE ORDER (PN)   * Helmet with outer cap in polycarbonate. * Expanded polystyrene inner liner for better shock absorption. * Interior with adjustable crown, for better heat dissipation * Liftable polycarbonate screen, minimum thickness 3mm * Seal at the top of the screen * Reinforcement metal bar on the top edge of the screen * 12 cm (+/- 10%) detachable PVC neck guard, attached by pressure to the rigid neck guard forming part of the shell, at the back of the helmet * Automatic loop closure * Removable chin strap on the jugular * 2 round ventilations on the ears for better hearing * 2 round ventilations on the front * One size fits all * Weight: 1.8 kg (+/- 10%)   QUANTITY: 50  ABIDJAN DELIVERY / COTE D’IVOIRE |  |  |  |
| 2.13 | MAINTENANCE OF THE ORDER (PN)   * Made of transparent polycarbonate thickness 4 mm minimum * Shock resistant * Ergonomic handle ambidextrous adjustment by velcro * Central horizontal foam strip to cushion shocks and improve user comfort * Weight: 4 kg (+/-15%) * Dimensions: H 100 cm x l 60 cm (+/-15%)   QUANTITY: 100  ABIDJAN DELIVERY / COTE D’IVOIRE |  |  |  |

Surname and first name: **<**.....................................................................................

Place and date: **<**.....................................................................................

Signature: **<**.....................................................................................

Company seal: **<**.....................................................................................